P-101

V-102

V-101

PI

V-101

Sample Vessel

Type: Vertical Cylindrical

Nominal Cap: 5 gal

Size: 12 in Dia 14.5 in High

Construction: HDPE

V-102

Effluent Vessel

Type: Vertical Cylindrical

Nominal Cap: 5 gal

Size: 12 in Dia 14.5 in High

Construction: HDPE

P-101

Transfer Pump

Type: Peristaltic

Nominal Cap: 85 GPD @ 100% PWR

Motor: 120 VAC / 60 Hz

Design Pressure: 25 psi

Manufacturer: Stenner Pump Company

Model: SVP4

¼”-Poly-Potable

¼”-Poly-Potable

¼”-Poly-Potable

MCV

Silver Antimicrobial Check valve

Type: Spring-loaded Inline Lift Check

Size: 1 in Dia 24 in High

Construction: 316 Stainless Steel

MCV